NBS Specification:



This product is associated with the following NBS Create clause:

90-05-20/306 Floor channels

NBS Specification:

NBS Buliding logo

This product is associated with the following NBS clauses:

[R11 Above ground foul drainage systems](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-External-DrainageSlotChannel)

* [315 FLOOR CHANNELS](https://www.ribaproductselector.com/Product.aspx?ci=23778&pr=KentStainless-External-DrainageSlotChannel)

Product Specification:

Curved Slot Channel

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Slot Channel

• Type: KSC125/200/100-10 /KSC125/250/100-10 /KSC125/300/100-10 /KSC175/250/100-10 /KSC175/300/100-10 /KSC175/350/100-10

• Material: Grade 1.4307 (304L) stainless steel /Grade 1.4404 (316L) stainless steel

• Loading: BS EN 124 B125 /BS EN 124 C250 /BS EN 124 D400

• Channel slot:

- Throat: Curved & Visible

- Type: Slot channel /Top slot channel

• Connectors: Channel connector /Drop connector /Silt trap connector

• End cap: Slot channel end cap

• Access cover: Recessed access box /Recessed access box with side fixed visible slot /Recessed access box with centre fixed visible slot

• Outlet point: Bottom /Side /End

Product Specification:

Curved Slot Channel

• Manufacturer: Kent Stainless

Web: www.kentstainless.com

Email: info@kentstainless.com

Tel: +44 (0) 800 376 8377

Fax: +353 53 914 1802

Address: Ardcavan Works, Ardcavan Co Wexford, Ireland

• Product reference: Slot Channel

• Type: KSC125/200/100-10 Curved

• Material: Grade 1.4404 (316L) stainless steel

• Loading: BS EN 124 B125

• Channel slot:

- Throat: Visible

- Type: Curved Slot channel

• Connectors: Channel connector

• End cap: Slot channel end cap

• Access cover: Recessed access box

• Outlet point: Bottom